**LFEV-Y6**

v0.7

**Lafayette College: Electrical and Computer Engineering**

Acceptance Test Plan: v0.7

Made by: Greg Flynn ‘17

Modified by: Waseh Ahmad ‘18

This document outlines all of the tests required to deliver LFEV-Y6. The plan is presented as an overview with the ATP number next to the test. This refers to the document that describes the test procedure. The requirements are from the SoW for 2018

08

**Fall**

Table of Contents

[ATP overviews 6](#_Toc479235589)

[Compliance Matrix 9](#_Toc479235590)

[Deliverables 11](#_Toc479235591)

[D000: PDR 11](#_Toc479235592)

[D001: CDR 11](#_Toc479235593)

[D002: User Manuals 11](#_Toc479235594)

[D003: Final Report and Maintenance Manual 11](#_Toc479235595)

[Final report 11](#_Toc479235596)

[Maintenance manual 12](#_Toc479235597)

[D004: ATP 13](#_Toc479235598)

[D005: ATR 13](#_Toc479235599)

[D007: Project Website 13](#_Toc479235600)

[D008: Final Presentation and Delivery 13](#_Toc479235601)

[D009: Conference Paper, Presentation, and Video 13](#_Toc479235602)

[D010: Project Poster 14](#_Toc479235603)

[D012: Software Maintainability Plan 14](#_Toc479235604)

[D013: Purchasing Report 14](#_Toc479235605)

[D014: Project Management and Status Letters 14](#_Toc479235606)

[Waived or modified requirements and questions 15](#_Toc479235607)

[ATP-01 checklist: Accumulator integration 16](#_Toc479235608)

[ATP-02 checklist: Charging Accumulator 17](#_Toc479235609)

[ATP-03 checklist: CAN Bus link 18](#_Toc479235610)

[ATP-04 checklist: Safety loop 19](#_Toc479235611)

[ATP-07 checklist: Shutdown 20](#_Toc479235612)

[ATP-08 checklist: GLV grounding 21](#_Toc479235613)

[ATP-09 checklist: Documentation 22](#_Toc479235614)

[TSV: Pacman 23](#_Toc479235615)

[TSV: AMS 23](#_Toc479235616)

[TSV: Pack 23](#_Toc479235617)

[TSV: Pack panel 24](#_Toc479235618)

[TSV: Bus bar 24](#_Toc479235619)

[TSV: Control panel PCB 24](#_Toc479235620)

[TSI: Container 25](#_Toc479235621)

[TSI: Front Panel 25](#_Toc479235622)

[TSI: Back Panel 25](#_Toc479235623)

[TSI: Bus bar 1 (AIR to connector) 26](#_Toc479235624)

[TSI: Bus bar 2 (connector to connector) 26](#_Toc479235625)

[TSI: PCB 26](#_Toc479235626)

[TSI: Dyno panel 27](#_Toc479235627)

[GLV: Container 28](#_Toc479235628)

[GLV: Front panel 28](#_Toc479235629)

[GLV: Back panel 28](#_Toc479235630)

[GLV: PCB 29](#_Toc479235631)

[GLV: Dyno panel 29](#_Toc479235632)

[Cooling: Assembly 29](#_Toc479235633)

[ATP-10 checklist: Hazmat 30](#_Toc479235634)

[ATP-11 checklist: Safety practice 30](#_Toc479235635)

[Wires 30](#_Toc479235636)

[Internal wiring 30](#_Toc479235637)

[W1 30](#_Toc479235638)

[W2 30](#_Toc479235639)

[W3 31](#_Toc479235640)

[W6 32](#_Toc479235641)

[W7 33](#_Toc479235642)

[W11 33](#_Toc479235643)

[W12 33](#_Toc479235644)

[W13 34](#_Toc479235645)

[W15 34](#_Toc479235646)

[W18 34](#_Toc479235647)

[W20 34](#_Toc479235648)

[W21 34](#_Toc479235649)

[W22 35](#_Toc479235650)

[W23 35](#_Toc479235651)

[W24 35](#_Toc479235652)

[W25 35](#_Toc479235653)

[W26 35](#_Toc479235654)

[W28 36](#_Toc479235655)

[W31 36](#_Toc479235656)

[W32 37](#_Toc479235657)

[W33 37](#_Toc479235658)

[W34 37](#_Toc479235659)

[W35 37](#_Toc479235660)

[W36 37](#_Toc479235661)

[Indicators 38](#_Toc479235662)

[IMD fault light 38](#_Toc479235663)

[Fault light 38](#_Toc479235664)

[AIRs Light 38](#_Toc479235665)

[Drive light 38](#_Toc479235666)

[Safety light 38](#_Toc479235667)

[Cruise light 39](#_Toc479235668)

[High Voltage Present light 39](#_Toc479235669)

[Grounded Low Voltage Present light 39](#_Toc479235670)

[Tractive System Energized Light 39](#_Toc479235671)

[Tractive System Active Light 39](#_Toc479235672)

[Brake light 40](#_Toc479235673)

[Buttons and switches 40](#_Toc479235674)

[FWD/REV switch 40](#_Toc479235675)

[Driver Reset 40](#_Toc479235676)

[Driver BRB 40](#_Toc479235677)

[Inertial switch 40](#_Toc479235678)

[Drive button 41](#_Toc479235679)

[Cruise button 41](#_Toc479235680)

[Scroll button 41](#_Toc479235681)

[Select button 41](#_Toc479235682)

[GLV Master Switch 41](#_Toc479235683)

[TSV Master Switch 42](#_Toc479235684)

[RHSBRB 42](#_Toc479235685)

[RHS MReset 42](#_Toc479235686)

[LHSBRB 42](#_Toc479235687)

[PCBs 43](#_Toc479235688)

[AMS 43](#_Toc479235689)

[Pacman 43](#_Toc479235690)

[TSI PCB 43](#_Toc479235691)

[GLV PCB 43](#_Toc479235692)

[Fuses 44](#_Toc479235693)

[Accumulator fuse 44](#_Toc479235694)

[Pacman fuse 44](#_Toc479235695)

[TSI precharge relay fuse 44](#_Toc479235696)

[GLV high current fuse 44](#_Toc479235697)

[GLV low current fuse 45](#_Toc479235698)

[Enclosures 46](#_Toc479235699)

[Pack 46](#_Toc479235700)

[TSI 46](#_Toc479235701)

[GLV 46](#_Toc479235702)

[ATP-12 checklist: Maintainability 47](#_Toc479235703)

[Software 47](#_Toc479235704)

[Pacman code 47](#_Toc479235705)

[AMS code 47](#_Toc479235706)

[VSCADA code 47](#_Toc479235707)

[Cell application code 48](#_Toc479235708)

[TSI code 48](#_Toc479235709)

[Remote software code 48](#_Toc479235710)

[Hardware 49](#_Toc479235711)

[Packs 49](#_Toc479235712)

[TSI 49](#_Toc479235713)

[GLV 49](#_Toc479235714)

[Cooling 49](#_Toc479235715)

[ATP-13 checklist: Demonstration 50](#_Toc479235716)

[ATP-14 checklist: Disposal 51](#_Toc479235717)

[Formula-Hybrid 2016 Electrical Inspection 52](#_Toc479235718)

[Accumulator Data 53](#_Toc479235719)

[ACCUMULATOR DATA FOR BATTERIES 53](#_Toc479235720)

[ACCUMULATOR DATA FOR CAPACITORS 53](#_Toc479235721)

[Preliminary Electrical Inspection (required prior to Mechanical Inspection) 54](#_Toc479235722)

[Operating Voltage 54](#_Toc479235723)

[Safety Circuit 54](#_Toc479235724)

[Indicator Operation 54](#_Toc479235725)

[TSMPs 54](#_Toc479235726)

[Ground Low Voltage 55](#_Toc479235727)

[Vehicle Grounding 55](#_Toc479235728)

[Tractive System Wiring 55](#_Toc479235729)

[TSMPs 55](#_Toc479235730)

[Indicators and Safety Labels 55](#_Toc479235731)

[Safety Components 55](#_Toc479235732)

[Full Inspection: Documentation/ESF 58](#_Toc479235733)

[Full Electrical: Inspection 61](#_Toc479235734)

[Full Electrical: Pouch Cells 63](#_Toc479235735)

[Final Demonstration 64](#_Toc479235736)

[Inspectors Reference 67](#_Toc479235737)

# ATP overviews

None of these tests can be viewed as completed until appropriate documentation has been uploaded to the webpage.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Item | Item description | Demonstrated Requirements | Successful Test Criteria | Verification Method |
| ATP-01 | Accumulator integration | R001aR001cR001dR001eR002aR002cR004a (TSV part)R005aR005b (Manual) | Packs power motor and all telemetry is recorded by VSCADA. Control by using the throttle.Verify by accelerating and looking at dash, pack screens, and log files remotely | Test |
| ATP-02 | Charging Accumulator | R001bR001gR002bR002h | Packs charge by the charging port and open the safety loopVSCADA reacts correctlyVerify by looking at the dash | Test |
| ATP-03 | CAN Bus link | R002aR002cR002dR002eR002fR002gR002jR002kR003a(8)R003dR004a (CAN Bus part)R005a (CAN Bus part)R005c (CAN Bus part)R007cR007d | DAQ by VSCADA of TSI, GLV, TSV, Cooling. Verify by looking at GLV Screen. All DAQ methods should happen simultaneously | Test |
| ATP-04 | Safety loop | R001gR002bR002cR002dR002kR002mR003bR003cR003dR004a (Safety loop part)R005c (IMD fault)R007b | Fault by:CrashingBRBIMDCoolingVSCADA limitPack faultThrottle faultBrake faultUser defined limit (halt)Pack chargingVerify by looking at the dash, the remote computer and the cellphone | Test |
| ~~ATP-06~~ | ~~24h endurance test~~ | ~~GPR006~~ | ~~At the end of all other tests leave the car running for 24h~~ | ~~Test~~ |
| ATP-07 | Shutdown | R002kR002i | VSCADA works after unexpected GLV shutdownAll hardware in safe statePacks stop powering motor with GLV shutdownTSI works after unexpected TSV shutdown | Test |
| ATP-08 | GLV grounding | R003a(2) | Ensure that there is only 1 connection between ground and chassis ground | Inspection |
| ATP-09 | Documentation | GRP001 | Complete and accurate documentation | Inspection |
| ATP-10 | Hazmat | GPR004 | No hazardous materials used | Analysis |
| ATP-11 | Safety practice | GPR005 | Good practice used for safety | Inspection |
| ATP-12 | Maintainability | GPR007 | Ensure that the project is maintainable | Analysis and test |
| ATP-13 | Demonstration | GPR011 | Have a video and demo setup | Inspection |
| ATP-14 | Disposal | GPR012 | Dispose of all materials as required | Inspection |

# Compliance Matrix

All requirements should also have a QA by each subsystem before integration.

|  |  |
| --- | --- |
| Requirement | Test(s) to demonstrate acceptance |
| R001a | ATP-01 |
| R001b | ATP-02 OR https://sites.lafayette.edu/ece492-sp16/files/2016/05/QAR001b.pdf |
| R001c | ATP-01  |
| R001d | ATP-01 |
| R001e | ATP-01 |
| R001f | https://sites.lafayette.edu/ece492-sp16/files/2016/05/QAR001e.pdf |
| R001g | ATP-02 |
| R002a | ATP-01 or ATP-03 |
| R002b | ATP-02 |
| R002c | ATP-01 OR ATP-03 OR ATP-04 |
| R002d | ATP-01 OR ATP-03 OR ATP-04 |
| R002e | ATP-03 |
| R002f | ATP-03 |
| R002g | ATP-03 |
| R002h | ATP-02 OR ATP-03 |
| R002i | ATP-02  |
| R002j | ATP-03 |
| R002k | ATP-03 |
| R002l | Waived |
| R002m | ATP-04 |
| R003a(1) | Any ATP |
| R003a(2) | ATP-08 |
| R003a(3) | QA by GLV |
| R003a(4) | ATP-02 |
| R003a(5) | ATP-02 |
| R003a(5) | ATP-02 |
| R003a(6) | ATP-02 |
| R003a(7) | ATP-02 |
| R003a(8) | ATP-03 |
| R003b | ATP-04 |
| R003c | QA by GLV |
| R003d | ATP-03 |
| R004a | ATP-01 AND ATP-03 AND ATP-04 |
| R004b | QA by Interconnect |
| R005a | ATP-01 AND ATP-03 |
| R005b | ATP-01 AND ATP-07 |
| R005c | ATP-04 |
| R005d | QA by TSI |
| R006 | Any ATP |
| R007a | QA by Cooling |
| R007b | ATP-04 |
| R007c | ATP-03 |
| R007d | ATP-03 |
| R007e | Waived |
| R007f | QA by Cooling |
| R007g | QA by Cooling |
| GPR001 | ATP-09 |
| GPR003 | Inspection |
| GPR004 | ATP-10 |
| GPR005 | ATP-11 (MTBF + power waived) |
| GPR006 | ATP-06 and ATP-11 |
| GRP007 | ATP-12 |
| GPR008 | ATP-09 |
| GPR011 | ATP-13 |
| GPR012 | ATP-14 |

# Deliverables

## D000: PDR

## <https://sites.lafayette.edu/ece492-sp18/files/2017/11/PDR_fall2017.pptx.pdf>

## D001: CDR

<https://sites.lafayette.edu/ece492-sp18/files/2018/03/Critical-Design-Review-1-1.pdf>

## D002: User Manuals

Note this is a checklist for the video

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| System | Getting started | FAQ | Functions and controls | Troubleshooting calibration and maintenance |
| TSI |  |  |  |  |
| TSV |  |  |  |  |
| GLV |  |  |  |  |
| Cooling |  |  |  |  |
| VSCADA |  |  |  |  |
| Dyno room |  |  |  |  |

Attach link to each of the videos to demonstrate competing the deliverable.

## D003: Final Report and Maintenance Manual

### Final report

|  |  |
| --- | --- |
| Check | Completed |
| Maintenance manuals completed |  |
| 3x DVD presented (or flash drive) |  |
| DVD artwork |  |
| ATP-09 completed |  |

Attach image of DVD or flash drive. Attach link to the final report with all of the documentation.

### Maintenance manual

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Part | TSI | TSV | GLV | Cool | VSCADA | Dyno | Andriod |
| Maintenance |  |  |  |  |  |  |  |
| Calibration |  |  |  |  |  |  |  |
| PCB schematic |  |  |  |  |  |  |  |
| PCB BOM |  |  |  |  |  |  |  |
| Mechanical drawing |  |  |  |  |  |  |  |
| Mechanical BOM |  |  |  |  |  |  |  |
| Block diagram |  |  |  |  |  |  |  |
| Wiring diagram |  |  |  |  |  |  |  |
| Gerber files |  |  |  |  |  |  |  |
| QA testing |  |  |  |  |  |  |  |
| Principal of operation |  |  |  |  |  |  |  |
| Software binaries |  |  |  |  |  |  |  |
| Software source |  |  |  |  |  |  |  |
| Software make file |  |  |  |  |  |  |  |
| ATP-12 completed |  |  |  |  |  |  |  |

Attach link to each of the maintenance manuals for this document.

## D004: ATP

|  |  |
| --- | --- |
| Check | Completed |
| Compliance matrix |  |
| Forms present |  |

<http://sites.lafayette.edu/ece492-sp17/testing/atp/>

## D005: ATR

|  |  |
| --- | --- |
| Check | Completed |
| All tests included |  |
| Test date for all tests |  |
| Photos as required |  |
| Tester named |  |
| Witness signature if available |  |
| Test results |  |

Attach link to the ATR.

## D007: Project Website

|  |  |
| --- | --- |
| Check | Completed |
| All documents as portable static documents (PDF/TXT/XML) |  |
| Original version present |  |
| Links to any cloud storage |  |

Attach link to the site for each document required.

## D008: Final Presentation and Delivery

|  |  |
| --- | --- |
| Check | Completed |
| GPR006 |  |
| GPR007 |  |
| GPR008 |  |
| GPR011 |  |
| D010 |  |
| Video for D009 |  |
| Video of GPR011 |  |
| Delivered per GPR012 |  |
| Any other items disposed per GPR012 |  |

Links to the final presentation provided. Link to the video.

## D009: Conference Paper, Presentation, and Video

Waived

## D010: Project Poster

Waived

## D012: Software Maintainability Plan

Waived by Professor Nadovich upon demonstration during CDR

## D013: Purchasing Report

|  |  |
| --- | --- |
| Check | Completed |
| Table for all purchases |  |
| Summary based on team |  |
| Summary based on week |  |

Link to purchasing reports provided.

## D014: Project Management and Status Letters

|  |  |
| --- | --- |
| Check | Completed |
| Status letter submitted |  |
| WBS delivered |  |

Link to WBS and status letter provided.

# Waived or modified requirements and questions

|  |  |
| --- | --- |
| Requirement | Reason |
| ~~R003a(4)~~ | ~~Cannot tell if GLV is from the battery or 24VDC~~ |
| ~~R002h~~ | ~~Cannot tell if GLV is from the battery or 24VDC~~ |
| ~~R007e~~ | ~~Waived~~ |
| ~~R005d~~ | ~~We’ve changed the switches~~ |
| ~~R002l~~ | ~~Waived~~ |
| ~~GPR003~~ | ~~Waived~~ |
| ~~GPR005~~ | ~~(Power and MTBF/MTTR waived)~~ |

# ATP-01 checklist: Accumulator integration

|  |  |
| --- | --- |
| Test | Pass |
| 1. Packs can deliver 200A through TSI
 |  |
| 1. Voltage measured at TSVMP is as expected
 |  |
| 1. Throttle controls RPM
 |  |
| 1. Throttle implausibility causes exit of drive mode
 |  |
| 1. Two moves required to enter drive mode
 |  |
| 1. Throttle and brake together prevent drive mode from starting
 |  |
| 1. Throttle and brake together exit drive mode
 |  |
| 1. TSAL lights come on when HV present outside packs
 |  |
| 1. TSEL lights come on when AIRS closed
 |  |
| 1. RTDS come on for 1-3 seconds when drive mode entered
 |  |
| 1. HV present light comes on when HV present
 |  |
| 1. Packs display telemetry on GLV screen
 |  |
| 1. Dyno can set the throttle
 |  |
| 1. Dyno can set the valve on the dyno
 |  |

Pass count: /14

|  |  |
| --- | --- |
| (Test) Variable to measure | Value |
| (a) Current according to current sensor |  |
| (a+l) Current according to pack 1 |  |
| (a+l) Current according to pack 2 |  |
| (a+l) Current according to pack 3 |  |
| (a+l) Current according to pack 4 |  |
| (a) Current according to TSI |  |
| (b) Voltage at TSVMP with 50A load |  |
| (b) Voltage at TSVMP with no draw |  |
| (c) Max RPM |  |
| (d) APPS1 voltage at implausibility |  |
| (d) APPS2 voltage at implausibility |  |
| (m) Max RPM |  |
| (n) Max torque |  |

# ATP-02 checklist: Charging Accumulator

|  |  |
| --- | --- |
| Test | Pass |
| 1. Safety loop opens when charging
 |  |
| 1. VSCADA shows that packs are charging
 |  |
| 1. Packs can be left charging after they are full
 |  |

Pass count: /4

Attach VSCADA data dump showing voltage and current with respect to time. This should be an excel document with data as well as a graph.

# ATP-03 checklist: CAN Bus link

|  |  |
| --- | --- |
| Test | Seen by VSCADA |
| Cell Temperature | /28 |
| Cell Voltage | /28 |
| Pack Current | /4 |
| Pack SoC | /4 |
| Pack Status | /4 |
| Pack Voltage | /4 |
| GLV Voltage |  |
| GLV SoC |  |
| GLV Current |  |
| GLV Temperature |  |
| Safety loop status |  |
| RPM gauge (Dyno) |  |
| Strain gauge |  |
| Throttle position |  |
| Brake status |  |
| IMD resistance |  |
| FWD/REV status |  |
| Precharge status |  |
| MC temp |  |
| MC current |  |
| Cooling temp in |  |
| Cooling flow |  |
| Cooling temp out |  |
| TSI temp |  |
| Speed |  |
| Safety loop status |  |

Pass count: /26

Attach excel document of data for VSCADA receiving data. Attach graphs from the android application. Attach screen shots of the remote computer in operation.

# ATP-04 checklist: Safety loop

|  |  |  |
| --- | --- | --- |
| Fault | Safety loop trip(Fault lit) | Seen on VSCADA |
| Driver resettable BRB |  |  |
| Non driver resettable BRB |  |  |
| Crash protection |  |  |
| Over temperature cooling |  |  |
| Under flow cooling |  |  |
| IMD fault |  |  |
| Cell overtemp  |  |  |
| Cell overcurrent |  |  |
| Cell overvoltage |  |  |
| Cell undervoltage |  |  |
| Brake overtravel |  |  |
| VSCADA defined violation |  |  |

Pass count: /24

Add logs from VSCADA showing faults. Add screen shots from the remote computer showing the faults. Add screen shots from the android application showing the faults.

# ATP-07 checklist: Shutdown

|  |  |
| --- | --- |
| Test | Pass |
| VSCADA powers up with no user input |  |
| GLV shutdown prevents TSV being present at TSVMP |  |
| TSVMS shutdown prevents TSV being present at TSVMP |  |
| VSCADA has recorded data up to the shutdown |  |
| TSVMS shutdown while under load does not create any issues |  |

Pass count: /5

Shutdown time (yyyy-mm-dd hh:mm:ss UTC):

Attach log from VSCADA showing data up until GLV shutdown.

# ATP-08 checklist: GLV grounding

Attach image of the grounding connection.

# ATP-09 checklist: Documentation

For every subassembly in a subsystem this checklist should be completed. I have attempted to capture them all but if there are parts not included they need to be added. Part numbers should go in a tree structure all the way down to commercial parts.

## TSV: Pacman

|  |  |
| --- | --- |
| Check | Pass |
| Unique part number |  |
| Document delivered to instructor |  |
| Document uploaded to website |  |
| Units defined on diagram clearly |  |
| Have a complete BOM with document if required |  |
| Part number on title block |  |
| Part number on file name |  |
| Part number on fabricated object |  |
| Lafayette Electrical and Computer Engineering marked |  |
| BOM had alternative or justification of only 1 supplier |  |

Pass count: /10

Part number:

Link:

## TSV: AMS

|  |  |
| --- | --- |
| Check | Pass |
| Unique part number |  |
| Document delivered to instructor |  |
| Document uploaded to website |  |
| Units defined on diagram clearly |  |
| Have a complete BOM with document if required |  |
| Part number on title block |  |
| Part number on file name |  |
| Part number on fabricated object |  |
| Lafayette Electrical and Computer Engineering marked |  |
| BOM had alternative or justification of only 1 supplier |  |

Pass count: /10

Part number:

Link:

## TSV: Pack

|  |  |
| --- | --- |
| Check | Pass |
| Unique part number |  |
| Document delivered to instructor |  |
| Document uploaded to website |  |
| Units defined on diagram clearly |  |
| Have a complete BOM with document if required |  |
| Part number on title block |  |
| Part number on file name |  |
| Part number on fabricated object |  |
| Lafayette Electrical and Computer Engineering marked |  |
| BOM had alternative or justification of only 1 supplier |  |

Pass count: /10

Part number:

Link:

## TSV: Pack panel

|  |  |
| --- | --- |
| Check | Pass |
| Unique part number |  |
| Document delivered to instructor |  |
| Document uploaded to website |  |
| Units defined on diagram clearly |  |
| Have a complete BOM with document if required |  |
| Part number on title block |  |
| Part number on file name |  |
| Part number on fabricated object |  |
| Lafayette Electrical and Computer Engineering marked |  |
| BOM had alternative or justification of only 1 supplier |  |

Pass count: /10

Part number:

Link:

## TSV: Bus bar

|  |  |
| --- | --- |
| Check | Pass |
| Unique part number |  |
| Document delivered to instructor |  |
| Document uploaded to website |  |
| Units defined on diagram clearly |  |
| Have a complete BOM with document if required |  |
| Part number on title block |  |
| Part number on file name |  |
| Part number on fabricated object |  |
| Lafayette Electrical and Computer Engineering marked |  |
| BOM had alternative or justification of only 1 supplier |  |

Pass count: /10

Part number:

Link:

## TSV: Control panel PCB

|  |  |
| --- | --- |
| Check | Pass |
| Unique part number |  |
| Document delivered to instructor |  |
| Document uploaded to website |  |
| Units defined on diagram clearly |  |
| Have a complete BOM with document if required |  |
| Part number on title block |  |
| Part number on file name |  |
| Part number on fabricated object |  |
| Lafayette Electrical and Computer Engineering marked |  |
| BOM had alternative or justification of only 1 supplier |  |

Pass count: /10

Part number:

Link:

## TSI: Container

|  |  |
| --- | --- |
| Check | Pass |
| Unique part number |  |
| Document delivered to instructor |  |
| Document uploaded to website |  |
| Units defined on diagram clearly |  |
| Have a complete BOM with document if required |  |
| Part number on title block |  |
| Part number on file name |  |
| Part number on fabricated object |  |
| Lafayette Electrical and Computer Engineering marked |  |
| BOM had alternative or justification of only 1 supplier |  |

Pass count: /10

Part number:

Link:

## TSI: Front Panel

|  |  |
| --- | --- |
| Check | Pass |
| Unique part number |  |
| Document delivered to instructor |  |
| Document uploaded to website |  |
| Units defined on diagram clearly |  |
| Have a complete BOM with document if required |  |
| Part number on title block |  |
| Part number on file name |  |
| Part number on fabricated object |  |
| Lafayette Electrical and Computer Engineering marked |  |
| BOM had alternative or justification of only 1 supplier |  |

Pass count: /10

Part number:

Link:

## TSI: Back Panel

|  |  |
| --- | --- |
| Check | Pass |
| Unique part number |  |
| Document delivered to instructor |  |
| Document uploaded to website |  |
| Units defined on diagram clearly |  |
| Have a complete BOM with document if required |  |
| Part number on title block |  |
| Part number on file name |  |
| Part number on fabricated object |  |
| Lafayette Electrical and Computer Engineering marked |  |
| BOM had alternative or justification of only 1 supplier |  |

Pass count: /10

Part number:

Link:

## TSI: Bus bar 1 (AIR to connector)

|  |  |
| --- | --- |
| Check | Pass |
| Unique part number |  |
| Document delivered to instructor |  |
| Document uploaded to website |  |
| Units defined on diagram clearly |  |
| Have a complete BOM with document if required |  |
| Part number on title block |  |
| Part number on file name |  |
| Part number on fabricated object |  |
| Lafayette Electrical and Computer Engineering marked |  |
| BOM had alternative or justification of only 1 supplier |  |

Pass count: /10

Part number:

Link:

## TSI: Bus bar 2 (connector to connector)

|  |  |
| --- | --- |
| Check | Pass |
| Unique part number |  |
| Document delivered to instructor |  |
| Document uploaded to website |  |
| Units defined on diagram clearly |  |
| Have a complete BOM with document if required |  |
| Part number on title block |  |
| Part number on file name |  |
| Part number on fabricated object |  |
| Lafayette Electrical and Computer Engineering marked |  |
| BOM had alternative or justification of only 1 supplier |  |

Pass count: /10

Part number:

Link:

## TSI: PCB

|  |  |
| --- | --- |
| Check | Pass |
| Unique part number |  |
| Document delivered to instructor |  |
| Document uploaded to website |  |
| Units defined on diagram clearly |  |
| Have a complete BOM with document if required |  |
| Part number on title block |  |
| Part number on file name |  |
| Part number on fabricated object |  |
| Lafayette Electrical and Computer Engineering marked |  |
| BOM had alternative or justification of only 1 supplier |  |

Pass count: /10

Part number:

Link:

## TSI: Dyno panel

|  |  |
| --- | --- |
| Check | Pass |
| Unique part number |  |
| Document delivered to instructor |  |
| Document uploaded to website |  |
| Units defined on diagram clearly |  |
| Have a complete BOM with document if required |  |
| Part number on title block |  |
| Part number on file name |  |
| Part number on fabricated object |  |
| Lafayette Electrical and Computer Engineering marked |  |
| BOM had alternative or justification of only 1 supplier |  |

Pass count: /10

Part number:

Link:

## GLV: Container

|  |  |
| --- | --- |
| Check | Pass |
| Unique part number |  |
| Document delivered to instructor |  |
| Document uploaded to website |  |
| Units defined on diagram clearly |  |
| Have a complete BOM with document if required |  |
| Part number on title block |  |
| Part number on file name |  |
| Part number on fabricated object |  |
| Lafayette Electrical and Computer Engineering marked |  |
| BOM had alternative or justification of only 1 supplier |  |

Pass count: /10

Part number:

Link:

## GLV: Front panel

|  |  |
| --- | --- |
| Check | Pass |
| Unique part number |  |
| Document delivered to instructor |  |
| Document uploaded to website |  |
| Units defined on diagram clearly |  |
| Have a complete BOM with document if required |  |
| Part number on title block |  |
| Part number on file name |  |
| Part number on fabricated object |  |
| Lafayette Electrical and Computer Engineering marked |  |
| BOM had alternative or justification of only 1 supplier |  |

Pass count: /10

Part number:

Link:

## GLV: Back panel

|  |  |
| --- | --- |
| Check | Pass |
| Unique part number |  |
| Document delivered to instructor |  |
| Document uploaded to website |  |
| Units defined on diagram clearly |  |
| Have a complete BOM with document if required |  |
| Part number on title block |  |
| Part number on file name |  |
| Part number on fabricated object |  |
| Lafayette Electrical and Computer Engineering marked |  |
| BOM had alternative or justification of only 1 supplier |  |

Pass count: /10

Part number:

Link:

## GLV: PCB

|  |  |
| --- | --- |
| Check | Pass |
| Unique part number |  |
| Document delivered to instructor |  |
| Document uploaded to website |  |
| Units defined on diagram clearly |  |
| Have a complete BOM with document if required |  |
| Part number on title block |  |
| Part number on file name |  |
| Part number on fabricated object |  |
| Lafayette Electrical and Computer Engineering marked |  |
| BOM had alternative or justification of only 1 supplier |  |

Pass count: /10

Part number:

Link:

## GLV: Dyno panel

|  |  |
| --- | --- |
| Check | Pass |
| Unique part number |  |
| Document delivered to instructor |  |
| Document uploaded to website |  |
| Units defined on diagram clearly |  |
| Have a complete BOM with document if required |  |
| Part number on title block |  |
| Part number on file name |  |
| Part number on fabricated object |  |
| Lafayette Electrical and Computer Engineering marked |  |
| BOM had alternative or justification of only 1 supplier |  |

Pass count: /10

Part number:

Link:

## Cooling: Assembly

|  |  |
| --- | --- |
| Check | Pass |
| Unique part number |  |
| Document delivered to instructor |  |
| Document uploaded to website |  |
| Units defined on diagram clearly |  |
| Have a complete BOM with document if required |  |
| Part number on title block |  |
| Part number on file name |  |
| Part number on fabricated object |  |
| Lafayette Electrical and Computer Engineering marked |  |
| BOM had alternative or justification of only 1 supplier |  |

Pass count: /10

Part number:

Link:

# ATP-10 checklist: Hazmat

|  |  |
| --- | --- |
| Check | Pass |
| All PCBs are RoHS |  |
| No NiCd/Pb-Acid batteries |  |
| Dispose pre 2002/96/EC WEEE Directive |  |

Attach link to hazmat documentation.

# ATP-11 checklist: Safety practice

## Wires

### Internal wiring

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| System | Clean cabling | No rats-nest | Color coded | Labeled |
| TSI |  |  |  |  |
| TSV |  |  |  |  |
| GLV |  |  |  |  |
| Cooling |  |  |  |  |

Attach pictures of the inside of each system to document.

### W1

Count: 3

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

Pass count: /9

Attach image as evidence

### W2

Count: 1

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

Pass count: /3

Attach image as evidence

### W3

Count: 1

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

Pass count: /3

Attach image as evidence

### W6

Count: 6

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

Pass count: /18

Attach image as evidence

### W7

Count: 1

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

Pass count: /3

Attach image as evidence

### W11

Count: 5

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

Pass count: /15

Attach image as evidence

### W12

Count: 1

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

Pass count: /3

Attach image as evidence

### W13

Count: 1

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

Pass count: /3

Attach image as evidence

### W15

Count: 1

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

Pass count: /3

Attach image as evidence

### W18

Count: 1

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

Pass count: /3

Attach image as evidence

### W20

Count: 1

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

Pass count: /3

Attach image as evidence

### W21

Count: 1

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

Pass count: /3

Attach image as evidence

### W22

Count: 1

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

Pass count: /3

Attach image as evidence

### W23

Count: 1

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

Pass count: /3

Attach image as evidence

### W24

Count: 1

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

Pass count: /3

Attach image as evidence

### W25

Count: 1

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

Pass count: /3

Attach image as evidence

### W26

Count: 1

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

Pass count: /3

Attach image as evidence

### W28

Count: 1

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

Pass count: /3

Attach image as evidence

### W31

Count: 7

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

Pass count: /21

Attach image as evidence

### W32

Count: 1

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

Pass count: /3

Attach image as evidence

### W33

Count: 1

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

Pass count: /3

Attach image as evidence

### W34

Count: 1

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

Pass count: /3

Attach image as evidence

### W35

Count: 1

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

Pass count: /3

Attach image as evidence

### W36

Count: 1

|  |  |
| --- | --- |
| Check | Pass |
| Wires correctly color coded |  |
| Cable labeled with gauge/max temperature/max voltage |  |
| Cable labeled with reference designator |  |

Pass count: /3

Attach image as evidence

## Indicators

### IMD fault light

|  |  |
| --- | --- |
| Check | Pass |
| Clear indicator of function |  |
| Red LED |  |
| Located in cockpit |  |
| Illuminates when IMD resistance is low |  |

Pass count: /4

Attach image of illuminated light

### Fault light

|  |  |
| --- | --- |
| Check | Pass |
| Clear indicator of function |  |
| Red LED |  |
| Located in cockpit |  |
| Illuminates when fault detected |  |

Pass count: /4

Attach image of illuminated light

### AIRs Light

|  |  |
| --- | --- |
| Check | Pass |
| Clear indicator of function |  |
| Green LED |  |
| Located in cockpit |  |
| Illuminates when AIRs closed detected |  |

Pass count: /4

Attach image of illuminated light

### Drive light

|  |  |
| --- | --- |
| Check | Pass |
| Clear indicator of function |  |
| Green LED |  |
| Located in cockpit |  |
| Illuminates when Drive mode entered |  |

Pass count: /4

Attach image of illuminated light

### Safety light

|  |  |
| --- | --- |
| Check | Pass |
| Clear indicator of function |  |
| Green LED |  |
| Located in cockpit |  |
| Illuminates when safety loop closed |  |

Pass count: /4

Attach image of illuminated light

### Safety System OK lights

|  |  |
| --- | --- |
| Check | Pass |
| Clear indicator of function |  |
| Orange LED |  |
| Located Either Side |  |
| Illuminates when safety loop closed |  |

Pass count: /4

Attach image of illuminated light

|  |  |
| --- | --- |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

### High Voltage Present light

|  |  |
| --- | --- |
| Check | Pass |
| Clear indicator of function |  |
| Red LED |  |
| Located in cockpit |  |
| Illuminates when HV outside of packs |  |

Pass count: /4

Attach image of illuminated light

### Grounded Low Voltage Present light

|  |  |
| --- | --- |
| Check | Pass |
| Clear indicator of function |  |
| Green LED |  |
| Located in cockpit |  |
| Illuminates when GLV powered |  |

Pass count: /4

Attach image of illuminated light

### Tractive System Active Lamp

|  |  |
| --- | --- |
| Check | Pass |
| 2Hz-5Hz frequency when on |  |
| Red Strobe |  |
| Mounted on the main hull, above driver helmet |  |
| Illuminates when AIRs closed |  |

Pass count: /4

Attach image of illuminated light

|  |  |
| --- | --- |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

### Brake light

|  |  |
| --- | --- |
| Check | Pass |
| 1 light present  |  |
| Red light |  |
| Located on dyno specific panel (will be on car in future) |  |
| Illuminates when brake pressed and GLV on |  |

Pass count: /4

Attach image of illuminated light

## Buttons and switches

### FWD/REV switch

|  |  |
| --- | --- |
| Check | Pass |
| Clearly labeled  |  |
| Key switch 2 position |  |
| Key can be removed in either state |  |
| Mounted on TSI box |  |

Pass count: /4

Attach image of button/switch:

### Driver Reset

|  |  |
| --- | --- |
| Check | Pass |
| Clearly labeled  |  |
| Green button |  |
| Momentary switch |  |
| Mounted in cockpit |  |

Pass count: /4

Attach image of button/switch:

### Driver BRB

|  |  |
| --- | --- |
| Check | Pass |
| Clearly labeled  |  |
| Red button |  |
| Latching button, twist to unlatch |  |
| Mounted in cockpit |  |

Pass count: /4

Attach image of button/switch:

### Inertial switch

|  |  |
| --- | --- |
| Check | Pass |
| Clearly labeled  |  |
| Inertial switch |  |
| Resettable by driver |  |
| Mounted in cockpit |  |

Pass count: /4

Attach image of button/switch:

### Drive button

|  |  |
| --- | --- |
| Check | Pass |
| Clearly labeled  |  |
| Tactile switch |  |
| Momentary button |  |
| Mounted in cockpit |  |

Pass count: /4

Attach image of button/switch:

|  |  |
| --- | --- |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

### Scroll button

|  |  |
| --- | --- |
| Check | Pass |
| Clearly labeled  |  |
| Tactile switch |  |
| Momentary button |  |
| Mounted in cockpit |  |

Pass count: /4

Attach image of button/switch:

### Record Button

|  |  |
| --- | --- |
| Check | Pass |
| Clearly labeled  |  |
| Tactile switch |  |
| Momentary button |  |
| Mounted in cockpit |  |

Pass count: /4

Attach image of button/switch:

### GLV Master Switch

|  |  |
| --- | --- |
| Check | Pass |
| Clearly labeled  |  |
| Red key switch |  |
| 2 position |  |
| Mounted on RHS panel |  |

Pass count: /4

Attach image of button/switch:

### TSV Master Switch

|  |  |
| --- | --- |
| Check | Pass |
| Clearly labeled  |  |
| Red key switch |  |
| 2 position |  |
| Mounted on RHS panel |  |

Pass count: /4

Attach image of button/switch:

### RHSBRB

|  |  |
| --- | --- |
| Check | Pass |
| Clearly labeled  |  |
| Red button |  |
| Latching button, twist to unlatch |  |
| Mounted on RHS panel near shoulder of Driver |  |

Pass count: /4

Attach image of button/switch:

### RHS MReset

|  |  |
| --- | --- |
| Check | Pass |
| Clearly labeled  |  |
| Green button |  |
| Momentary switch |  |
| Mounted on RHS panel near shoulder of Driver |  |

Pass count: /4

Attach image of button/switch:

### LHSBRB

|  |  |
| --- | --- |
| Check | Pass |
| Clearly labeled  |  |
| Red button |  |
| Latching button, twist to unlatch |  |
| Mounted on LHS panel |  |

Pass count: /4

Attach image of button/switch:

## PCBs

### AMS

|  |  |
| --- | --- |
| Check | Pass |
| Silkscreens marking reference designators |  |
| Silkscreens marking power and critical signals |  |
| Silkscreen showing Lafayette College, Made in USA, Electrical and Computer Engineering, part number |  |
| Space for serial number |  |
| Bottom copper has part number and rev |  |

Pass count: /5

Attach picture of front and back of PCB.

### Pacman

|  |  |
| --- | --- |
| Check | Pass |
| Silkscreens marking reference designators |  |
| Silkscreens marking power and critical signals |  |
| Silkscreen showing Lafayette College, Made in USA, Electrical and Computer Engineering, part number |  |
| Space for serial number |  |
| Bottom copper has part number and rev |  |

Pass count: /5

Attach picture of front and back of PCB.

### TSI PCB

|  |  |
| --- | --- |
| Check | Pass |
| Silkscreens marking reference designators |  |
| Silkscreens marking power and critical signals |  |
| Silkscreen showing Lafayette College, Made in USA, Electrical and Computer Engineering, part number |  |
| Space for serial number |  |
| Bottom copper has part number and rev |  |

Pass count: /5

Attach picture of front and back of PCB.

### GLV PCB

|  |  |
| --- | --- |
| Check | Pass |
| Silkscreens marking reference designators |  |
| Silkscreens marking power and critical signals |  |
| Silkscreen showing Lafayette College, Made in USA, Electrical and Computer Engineering, part number |  |
| Space for serial number |  |
| Bottom copper has part number and rev |  |

Pass count: /5

Attach picture of front and back of PCB.

## Fuses

### Accumulator fuse

|  |  |
| --- | --- |
| Check | Pass |
| UL listed socket as a holder |  |
| 5 spares |  |
| Easy to access |  |

Pass count: /3

Holder part number:

Fuse part number:

Attach image of fuse location

### Pacman fuse

|  |  |
| --- | --- |
| Check | Pass |
| UL listed socket as a holder |  |
| 5 spares |  |
| Easy to access |  |

Pass count: /3

Holder part number:

Fuse part number:

Attach image of fuse location

### TSI precharge relay fuse

|  |  |
| --- | --- |
| Check | Pass |
| UL listed socket as a holder |  |
| 5 spares |  |
| Easy to access |  |

Pass count: /3

Holder part number:

Fuse part number:

Attach image of fuse location

### GLV high current Circuit Breaker

|  |  |
| --- | --- |
| Check | Pass |
| UL listed socket as a holder |  |
| 5 spares |  |
| Easy to access |  |

Pass count: /3

Holder part number:

Fuse part number:

Attach image of fuse location

### GLV low current circuit Breaker

|  |  |
| --- | --- |
| Check | Pass |
| UL listed socket as a holder |  |
| 5 spares |  |
| Easy to access |  |

Pass count: /3

Holder part number:

Fuse part number:

Attach image of fuse location

## Enclosures

### Pack

|  |  |
| --- | --- |
| Check | Pass |
| Access panel present |  |
| Pilot lights and indicators present |  |
| All interconnect cables have at least 1 return signal |  |
| PCBs are not mounted directly to enclosure |  |
| Enclosures are grounded if they are conductive |  |
| Labeled internally and externally |  |

Pass count: /6

Attach 6 images of enclosures (All views)

### TSI

|  |  |
| --- | --- |
| Check | Pass |
| Access panel present |  |
| Pilot lights and indicators present |  |
| All interconnect cables have at least 1 return signal |  |
| PCBs are not mounted directly to enclosure |  |
| Enclosures are grounded if they are conductive |  |
| Labeled internally and externally |  |

Pass count: /6

Attach 6 images of enclosures (All views)

### GLV

|  |  |
| --- | --- |
| Check | Pass |
| Access panel present |  |
| Pilot lights and indicators present |  |
| All interconnect cables have at least 1 return signal |  |
| PCBs are not mounted directly to enclosure |  |
| Enclosures are grounded if they are conductive |  |
| Labeled internally and externally |  |

Pass count: /6

Attach 6 images of enclosures (All views)

# ATP-12 checklist: Maintainability

## Software

### Pacman code

|  |  |
| --- | --- |
| Check | Pass |
| Version controlled |  |
| Can startup with no input from the user |  |
| Have an install script (.exe/make/RPM) |  |
| Configurable without requiring a recompile |  |
| Data stored in a well-supported format |  |
| Any files that grow should be automatically trimmed |  |
| A procedure for backing up data |  |
| Passwords should be avoided |  |
| If a port is needed it should enumerate automatically |  |

Pass count: /9

### AMS code

|  |  |
| --- | --- |
| Check | Pass |
| Version controlled |  |
| Can startup with no input from the user |  |
| Have an install script (.exe/make/RPM) |  |
| Configurable without requiring a recompile |  |
| Data stored in a well-supported format |  |
| Any files that grow should be automatically trimmed |  |
| A procedure for backing up data |  |
| Passwords should be avoided |  |
| If a port is needed it should enumerate automatically |  |

Pass count: /9

### VSCADA code

|  |  |
| --- | --- |
| Check | Pass |
| Version controlled |  |
| Can startup with no input from the user |  |
| Have an install script (.exe/make/RPM) |  |
| Configurable without requiring a recompile |  |
| Data stored in a well-supported format |  |
| Any files that grow should be automatically trimmed |  |
| A procedure for backing up data |  |
| Passwords should be avoided |  |
| If a port is needed it should enumerate automatically |  |

Pass count: /9

### Cell application code

|  |  |
| --- | --- |
| Check | Pass |
| Version controlled |  |
| Can startup with no input from the user |  |
| Have an install script (.exe/make/RPM) |  |
| Configurable without requiring a recompile |  |
| Data stored in a well-supported format |  |
| Any files that grow should be automatically trimmed |  |
| A procedure for backing up data |  |
| Passwords should be avoided |  |
| If a port is needed it should enumerate automatically |  |

Pass count: /9

### TSI code

|  |  |
| --- | --- |
| Check | Pass |
| Version controlled |  |
| Can startup with no input from the user |  |
| Have an install script (.exe/make/RPM) |  |
| Configurable without requiring a recompile |  |
| Data stored in a well-supported format |  |
| Any files that grow should be automatically trimmed |  |
| A procedure for backing up data |  |
| Passwords should be avoided |  |
| If a port is needed it should enumerate automatically |  |

Pass count: /9

|  |  |
| --- | --- |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

## Hardware

### Packs

|  |  |
| --- | --- |
| Check | Pass |
| Recommended list of spare hardware |  |
| Basic troubleshooting guidelines for a beginner |  |
| Advance troubleshooting for an expert |  |
| A beginner can diagnose a simple problem (loose connector) |  |
| An expert can diagnose a complex problem (TBA) |  |

Pass count: /5

Link to documentation:

### TSI

|  |  |
| --- | --- |
| Check | Pass |
| Recommended list of spare hardware |  |
| Basic troubleshooting guidelines for a beginner |  |
| Advance troubleshooting for an expert |  |
| A beginner can diagnose a simple problem (loose connector) |  |
| An expert can diagnose a complex problem (TBA) |  |

Pass count: /5

Link to documentation:

### GLV

|  |  |
| --- | --- |
| Check | Pass |
| Recommended list of spare hardware |  |
| Basic troubleshooting guidelines for a beginner |  |
| Advance troubleshooting for an expert |  |
| A beginner can diagnose a simple problem (loose connector) |  |
| An expert can diagnose a complex problem (TBA) |  |

Pass count: /5

Link to documentation:

### Cooling

|  |  |
| --- | --- |
| Check | Pass |
| Recommended list of spare hardware |  |
| Basic troubleshooting guidelines for a beginner |  |
| Advance troubleshooting for an expert |  |
| A beginner can diagnose a simple problem (loose connector) |  |
| An expert can diagnose a complex problem (TBA) |  |

Pass count: /5

Link to documentation:

# ATP-13 checklist: Demonstration

|  |  |
| --- | --- |
| Check | Pass |
| 1080p compressed video supplied |  |
| Video ~5min in length |  |
| Slideshow of final project |  |
| Demonstration of final project |  |
| Standalone self-contained display provided |  |

Pass count: /5

Attach link to video, slides and image of display.

# ATP-14 checklist: Disposal

|  |  |
| --- | --- |
| Check | Pass |
| All materials stored in the same room |  |
| Webpage updated to a final version |  |
| Old material removed from webpage |  |
| Test equipment returned |  |
| Trash cleaned in 400 and 401 |  |
| Items disposed in accordance with Hazmat procedures |  |
| Paper recycled |  |
| Webpage matches demonstration |  |

Pass count: /8

Attach link to disposal procedure. Attach image of clean lab at the end.

Figure - FSM for TSI



Figure - ATP-01 block diagram



Figure 3 - ATP-02 block diagram

Figure - ATP-03 block diagram



Figure - ATP-04 block diagram

